|  |
| --- |
| **ProduCt CategorY rULES fOR BUILDING RELATED  PRODUCTS AND SERVICES**  **as per ISO 14025 and EN 15804+A2** |
| **for preparation of EPDs (Environmental Product Declarations)  according to the EPD programme of the BAU EPD GmbH** |
|  |
| **www.bau-epd.at**  **Part B: Requirements on the EPD for**  **Expanded polystyrene foam (EPS)**  **Extruded polystyrene foam (XPS)**  PCR-Code: 2.22.2.1 Date 2023-01-27 |

****

**Imprint**

**Publisher:**

Bau EPD GmbH

Seidengasse 13/3

A-1070 Vienna

Austria

<http://www.bau-epd.at>

[office@bau-epd.at](mailto:office@bau-epd.at)

© Bau EPD GmbH

Picture credits frontpage: Austrotherm GmbH

**Tracking of versions**

|  |  |  |
| --- | --- | --- |
| Version | Comments | Date of changes |
| 8.0 | New structure following decisions of TAC from 2017-05-11, adaptations following resolutions from TAC in autumn 2016 and 2017. | 2017-08-17 |
| 9.0 | Changes following decisions of TAC since last publication. Changes on occasion of verification of PCR for concrete and concrete elements as well as resulting from working out the PCR for steel reinforcement. Changes to be made in all PCR B parts as well as some editorial chances. Index now included. | 2019-07-06 |
| 10.0 | Adaptation as per EN 15804:2019+A2:2019; adaptation of rules for declaration of geographical representativity | 2020-11-05 |
| 11.0 | Public version for interested parties after approval of PCR review panel. | 2021-01-12 |
| 12.0 | Consideration of comments, approval for EPD creation | 2021-04-07 |
| 13.0 | Adaptation tables module B and C, minor editorial changes | 2021-08-27 |
| 14.0 | Change ECO Platform logo, note to photographic rights, minor editorial changes (created by SR, checked by FG and approved by SR) | 2021-11-27 |
| 15.0 | **Addition of accreditation mark, change owner, publisher, holder of declaration, specification of CF factors, editorial changes, title page EPD declaration of Energy Mix Approach,**  **(created by SR, checked by FG and approved by SR)** | **2023-01-27** |

Contents

[1. Scope 5](#_Toc517348316)

[Requirements on the layout of the EPD 5](#_Toc517348317)

[Content of the EPD 5](#_Toc517348318)

[1. General information 7](#_Toc517348319)

[2. Product 9](#_Toc517348320)

[2.1 General product description 9](#_Toc517348321)

[2.2 Application field 9](#_Toc517348322)

[2.3 Standards, guidelines and regulations relevant for the product 10](#_Toc517348323)

[2.4 Technical data 11](#_Toc517348324)

[2.5 Basic/auxiliary materials 14](#_Toc517348325)

[2.6 Production 15](#_Toc517348326)

[2.7 Packaging 15](#_Toc517348327)

[2.8 Conditions of delivery 15](#_Toc517348328)

[2.9 Transport 15](#_Toc517348329)

[2.10 Processing/ installation 15](#_Toc517348330)

[2.11 Use stage 16](#_Toc517348331)

[2.12 Reference service life (RSL) 16](#_Toc517348332)

[2.13 Reuse and recycling 16](#_Toc517348333)

[2.14 Disposal 16](#_Toc517348334)

[2.15 Further information 16](#_Toc517348335)

[3. LCA: Calculation rules 18](#_Toc517348336)

[3.1 Declared unit/ Functional unit 18](#_Toc517348337)

[3.2 System boundary 18](#_Toc517348338)

[3.3 Flow chart of processes/stages in the life cycle 20](#_Toc517348339)

[3.4 Estimations and assumptions 20](#_Toc517348340)

[3.5 Cut-off criteria 20](#_Toc517348341)

[3.6 Data sources 20](#_Toc517348342)

[3.7 Data quality 20](#_Toc517348343)

[3.8 Reporting period 20](#_Toc517348344)

[3.9 Allocation 20](#_Toc517348345)

[3.10 Comparability 20](#_Toc517348346)

[4. LCA: Szenarios and additional technical information 21](#_Toc517348347)

[4.1 A1-A3 product stage 21](#_Toc517348348)

[4.2 A4-A5 Construction process stage 21](#_Toc517348349)

[4.3 B1-B7 use stage 21](#_Toc517348350)

[4.4 C1-C4 End-of-Life stage 23](#_Toc517348351)

[4.5 D Potential of reuse and recycling 24](#_Toc517348352)

[5. LCA: results 24](#_Toc517348353)

[6. LCA: Interpretation 28](#_Toc517348354)

[7. Literature 29](#_Toc517348355)

[8. Directory and Glossary 29](#_Toc517348356)

[8.1 List of figures 29](#_Toc517348357)

[8.2 List of tables 29](#_Toc517348358)

[8.3 Abbreviations 30](#_Toc517348359)

# Scope

This document contains the **Requirements on an Environmental Product Declaration (EPD)** as per EN 15804 and ISO 14025 and requirements of Bau EPD GmbH.

The document applies to factory-made insulating materials made of expanded polystyrene foam (EPS) and extruded polystyrene foam (XPS) in accordance with the following standards:

• ÖNORM EN 13163 Thermal insulation products for buildings - Factory made expanded polystyrene (EPS) products - Specification

• ÖNORM EN 13164 Thermal insulation products for buildings - Factory made products made of extruded polystyrene (XPS) - Specification

• ÖNORM EN 14307 Thermal insulation materials for technical building equipment and for operational systems in industry - Factory-made products made of extruded polystyrene foam (XPS) - Specification ÖNORM EN 14309 Thermal insulation materials for building technology and for operational systems - Factory-made products made of expanded polystyrene (EPS) – specification

* ÖNORM EN 16025-1 Thermal insulation products for thermal and/or acoustic insulation in buildings - Bonded EPS fillers - Part 1 - Requirements for factory premixed EPS dry mortar

The requirements on the EPD include:

* Requirements from EN ISO 14025
* Requirements on the EN 15804 standard as a European core EPD
* Requirements from EN 16783 as complementary product PCR for insulating materials
* Complementary requirements on EPD of Bau EPD GmbH

The calculation rules for the Life Cycle Assessment and Requirements on the project report are specified in a separate document – “Management System Handbook chapter 5” of Bau EPD GmbH.

# Requirements on the layout of the EPD

Bau-EPD GmbH determines the following features with regard to the layout of the EPD:

* The document on hand defines the format template for EPD-document that is to fill in (Word file „Format template EPD Bau EPD GmbH“, download at [www.bau-epd.at](http://www.bau-epd.at)).
* The content of an EPD is not limited in length of text.
* The layout of the front page of the EPD is defined and picture material must be accorded with Bau EPD GmbH (not more than 4 MB).
* On the last page of the EPD the publishing institution as well as the programme operator (Bau EPD GmbH in both cases), the LCA practitioner and owner of the declaration must be indicated with a logo and full address (including telephone number, fax number, email and website).
* Generally the font „Calibri“ must be used.
* In addition to the EPD as Microsoft Word format an Excel-document (BAU EPD M-DOCUMENT 8- excel-file for electronic data transfer Editor baubook ECO Platform) must be created including the result tables for electronic transfer and complying to EN 15942 (ITM Matrix). The templates of Bau EPD GmbH must be used, for these tables also serve to forward data to database owners (ECO Platform/ECO Portal, OEKOBAUDAT and BAUBOOK).

# Content of the EPD

The following format template respective guidance describes the required structure of the EPD document including the **required content for each individual chapter**.

In addition to that, this document is giving **specific notes for the creation of an EPD of mineral insulating** and **specific LCA calculation rules for EPS and XPS insulating materials** that must be considered when creating the EPD and underlying LCA study.

Parts of the content that are considered as additional information of optional character (=not required as per international standard and/or guidelines from ECO Platform) are marked in lilac colour. This information is free to choose whether to declare or not and indications can be delivered by the owner of the declaration on optional basis.

Legend:

Blue: required content for each chapter

Turquoise: specific requirements for EPD of materials from the scope of the PCR

Green: specific LCA rules for EPD of material from the scope of the PCR

Violet: additional information of optional character

|  |
| --- |
| **EPD - ENVIRONMENTAL PRODUCT DECLARATION** |
| **As per ISO 14025 and EN 15804** |
|  |
| **OWNER AND Publisher** **Bau EPD GmbH, A-1070 Wien, Seidengasse 13/3, www.bau-epd.at**  **Programme Operator Bau EPD GmbH, A-1070 Wien, Seidengasse 13/3, www.bau-epd.at**  **Holder of the Declaration Name of declaration holder**  **Declaration Number To be accorded with Bau EPD GmbH**  **Issue Date Date**  **Valid To Date**  **NUMBER OF DATASETS Number**  **ENERGY MIX APPROACH MARKET BASED APPROACH** |

**Name and description of product**

**Name of declaration owner**

**picture**

**To be accorded with declaration owner and Bau EPD GmbH**

**(Note: photographic rights must be clarified and cited)**

**Company logo of declaration owner**

Contents:

[**Content of the EPD 5**](#_Toc517348318)

[1. General information 7](#_Toc517348319)

[2. Product 9](#_Toc517348320)

[2.1 General product description 9](#_Toc517348321)

[2.2 Application field 9](#_Toc517348322)

[2.3 Standards, guidelines and regulations relevant for the product 10](#_Toc517348323)

[2.4 Technical data 11](#_Toc517348324)

[2.5 Basic/auxiliary materials 14](#_Toc517348325)

[2.6 Production 15](#_Toc517348326)

[2.7 Packaging 15](#_Toc517348327)

[2.8 Conditions of delivery 15](#_Toc517348328)

[2.9 Transport 15](#_Toc517348329)

[2.10 Processing/ installation 15](#_Toc517348330)

[2.11 Use stage 16](#_Toc517348331)

[2.12 Reference service life (RSL) 16](#_Toc517348332)

[2.13 Reuse and recycling 16](#_Toc517348333)

[2.14 Disposal 16](#_Toc517348334)

[2.15 Further information 16](#_Toc517348335)

[3. LCA: Calculation rules 18](#_Toc517348336)

[3.1 Declared unit/ Functional unit 18](#_Toc517348337)

[3.2 System boundary 18](#_Toc517348338)

[3.3 Flow chart of processes/stages in the life cycle 20](#_Toc517348339)

[3.4 Estimations and assumptions 20](#_Toc517348340)

[3.5 Cut-off criteria 20](#_Toc517348341)

[3.6 Data sources 20](#_Toc517348342)

[3.7 Data quality 20](#_Toc517348343)

[3.8 Reporting period 20](#_Toc517348344)

[3.9 Allocation 20](#_Toc517348345)

[3.10 Comparability 20](#_Toc517348346)

[4. LCA: Szenarios and additional technical information 21](#_Toc517348347)

[4.1 A1-A3 product stage 21](#_Toc517348348)

[4.2 A4-A5 Construction process stage 21](#_Toc517348349)

[4.3 B1-B7 use stage 21](#_Toc517348350)

[4.4 C1-C4 End-of-Life stage 23](#_Toc517348351)

[4.5 D Potential of reuse and recycling 24](#_Toc517348352)

[5. LCA: results 24](#_Toc517348353)

[6. LCA: Interpretation 28](#_Toc517348354)

[7. Literature 29](#_Toc517348355)

[8. Directory and Glossary 29](#_Toc517348356)

[8.1 List of figures 29](#_Toc517348357)

[8.2 List of tables 29](#_Toc517348358)

[8.3 Abbreviations 30](#_Toc517348359)

# General information

|  |  |
| --- | --- |
| **Product name**  Name and description of product | **Declared Product / Declared Unit**  Description of the declared product and declared unit/functional unit  **Number of datasets in EPD Document(s):** XX  **Range of validity**  The products considered in the data of the life cycle assessment and for which the declaration applies must be named.  In the case of an average EPD, this type of EPD must be pointed out.  The representativeness of the declaration must be shown with regard to the production volume covered by the life cycle assessment and the technology used. Likewise, the range of fluctuation of the product group considered, must be specified in the interpretation. |
| **Declaration number**  To be accorded with Bau EPD GmbH |
| **Declaration data**  Specific data  Average data |
| **Declaration based on:**  MS-HB version dated dd.mm.yyyy:  Name of PCR  PCR Code  Version  (PCR tested and approved by the independent expert committee  = PKR-Gremium)  The owner of the declaration is liable for the underlying information and evidence; Bau EPD GmbH is not liable with respect to manufacturer  information, life cycle assessment data and evidence. |
| **Type of Declaration as per EN 15804**  From cradle to ... ..... | **Database, Software, Version**  Declaration of backround database, Software used and both its versions  **Version Characterisation Factors:** Quelle, Version |
| **Author of the Life Cycle Assessment**  Name of the author  Institution, Address  website | **The CEN standard EN 15804:2014+A1 serves as the core-PCR.**  **Independent verification of the declaration according to ISO 14025:2010**  internally  externally  **Verifier 1:** Name  **Verifier 2:** Name |
| **Holder of the Declaration**  Name of the manufacturer/owner  Institution, Address  website | **Owner, Publisher and Programme Operator**  Bau EPD GmbH  Seidengasse 13/3  1070 Vienna  Austria |

**DI (FH) DI DI Sarah Richter**

Head of Conformity Assessment Body

**Academic Title Name** **Academic Title Name,**

Verifier Verifier

**Note:** EPDs from similar product groups from different programmes might not be comparable.

# Product

## General product description

For the product description the characteristics of the declared product must be described. In case of average EPD (“sector or branch” EPD) all declared products must be described separately.

Indications for the general product description:

* Separate description of products/materials for each product standard applicable, citing the product types and names.
* Description of characteristic components.
* All factory locations for the respective product categories must be declared, alternatively a reference can be made to an overview in an appendix (mandatory information in the project report, voluntary information in the EPD document)

**Specific notes for the creation of an EPD for EPS and XPS insulating materials:**

* Separate description of EPS and XPS insulating materials for each product standard applicable
* The declared product is…

## Application field

The use and application purpose of the named products are to specify. The individual applications (including functions) must be declared as a text or table format.

**Example as a table format:**

For products, the areas of application according to ÖNORM EN 16783 must be ticked in the following table:

Table 1: Applications for thermal insulation in buildings according to ÖNORM EN 16783 - Annex A

|  |  |  |  |
| --- | --- | --- | --- |
| **Area of application** | **Designation** | **Application description** | **Application specific product(s)** |
| Ceiling, Roof,  floor | DAD | External insulation of warm pitched roof or ceiling insulation, protected against weathering, insulation under cover | X |
| DAA | External insulation of flat roof or ceiling, protected against weathering, insulation under water proofing | X |
| DUK | External insulation of the roof, exposed to the weather (inverted roof) | X |
| DZ | Insulation between the rafters, two-shell roof, top floor ceiling not readily walkable but accessible | X |
| DI | Interior insulation of the ceiling (underside) or the roof, insulation under the rafters / supporting structure, false ceiling etc. | X |
| DEO | Interior insulation of the ceiling or floor plate (top side) below floor screed without acoustic dampening requirements | X |
| DES | Interior insulation of the ceiling or floor plate (top side) below screed with acoustic dampening requirements | X |
| VR | Thermal insulation between rafters, ventilated space directly above thermal insulation | X |
| Wall | WAB | External wall insulation behind covers (incl. ventilated façades) | X |
| WAA | External wall insulation behind seal | X |
| WAP | External Thermal Insulation Composite System with render | X |
| WZ | Insulation of double-leaf walls, cavity wall insulation | X |
| WH | Insulation of wood frame and wood panel construction | X |
| WI | Interior wall insulation (insulation of walls from inside) | X |
| WTH | Insulation between the house partition walls with sound insulation requirements (between adjacent houses) | X |
| WTR | Insulation of partitioning walls (within one house) | X |
| Perimeter | PW | External thermal insulation of walls in contact with soil (outside of the water proofing) | X |
| PB  FI | External thermal insulation under the floor panel in contact with soil outside of water proofing) | X |

Table 2: Applications for thermal insulation in building equipment, industry and civil engineering as per ÖNORM EN 16783 – Annex A

|  |  |  |  |
| --- | --- | --- | --- |
| **Area of application** | **Designation** | **Application description** | **Application specific product(s)** |
| Building equipment | BEF | Flat application | X |
| BEL | Linear (e.g. pipe insulation) | X |
| Industry | IF | Flat application | X |
| IL | Linear (e.g. pipe insulation) | X |
| Civil engineering | CI | Civil Engineering | X |
| LWF | Light-weight fill | X |
| ILB | Insulation under load-bearing structure | X |

## Standards, guidelines and regulations relevant for the product

The respective standard and/or general technical approval or comparable national regulation can be indicated.

Optional: Documentation under the frame of CE -certification such as certificates of constancy of performance, certificates of conformity of the internal production control on the manufacturer’s site, Declarations of performance, Official certificates of registration, European Technical Assessments or Technical permissions of construction industry can be cited.

**Specific notes for the creation of an EPD for EPS and XPS insulating materials:**

The standards regulating EPS and XPS insulating materials must be cited (i.e. standards, guidelines, other regulations)

Examples for product standards for EPS and XPS insulating materials in Austria are illustrated in table 3.

Table : Product specific standards

|  |  |
| --- | --- |
| **Standard** | **Title** |
| ÖNORM EN 13163:2013-03-01 | Thermal insulation products for buildings - Factory made expanded polystyrene (EPS) products - Specification |
| ÖNORM EN 14309:2016 02 15 | Thermal insulation products for building equipment and industrial installations - Factory made expanded polystyrene (EPS) products - Specification |

## Technical data

For products carrying a CE marking as per Construction Products Regulation (CPR) the EPD must declare at least the same technical data as required and indicated in the declaration of performance of the manufacturer. What kind of data is required in each individual case is to learn from the document underlying the CE marking: any Harmonized European Standard or European Technical Assessment (ETA).

Additional technical data must be listed if relevant for product distinction or specification.

**Specific notes for the creation of an EPD for EPS and XPS insulating materials:**

Product designation codes of the declared products must be given.

If relevant for the declared product, the following technical construction data in the delivery status must be provided with reference to the testing standard.

For declared products according to ÖNORM EN 13163, if applicable, the following technical data with reference to the test standard must be given:

Table 4: Technical characterizations for products as per ÖNORM EN 13163

|  |  |  |
| --- | --- | --- |
| **Characterization** | **Value** | **Unit** |
| thermal resistance  thermal conductivity  Design value of thermal conductivity |  | m²·K/W  W/m·K  W/m·K |
| Raw density1) or raw density range |  | kg/m3 |
| Euro class of fire behavior according to ÖNORM EN 13501-1 | E |  |
| Dimensional stability in normal climate | level |  |
| Dimensional stability under defined temperature and humidity conditions | class |  |
| Compressive stress at 10% compression | level |  |
| flexural strength | level |  |
| Tensile strength perpendicular to the plane of the plate | level |  |
| Deformation under defined pressure and temperature stress | level |  |
| Long-term creep behavior under compressive stress | level |  |
| shear strength and/or shear modulus | level |  |
| Relative deformation under cyclic loading | level |  |
| Water absorption during long-term immersion | level |  |
| Long-term water absorption by diffusion | level |  |
| Resistance to freeze-thaw cycling after water absorption after long-term total immersion | level |  |
| Resistance to freeze-thaw cycling after long-term water absorption by diffusion | level |  |
| Water vapor diffusion resistance factor µ or water vapor diffusion resistance Z | level | -  m²·s·Pa/kg |
| Dynamic Stiffness | level |  |
| compressibility | level |  |
| Long-term thickness reduction | level |  |

1) Mean bulk density

Für deklarierte Produkte gemäß ÖNORM EN 14309 sind, wenn zutreffend, folgende technische Daten unter Verweis auf die Prüfnorm anzuführen:

Table 5: Technical data for products as per ÖNORM EN 14309

|  |  |  |
| --- | --- | --- |
| **Characterization** | **Value** | **Unit** |
| thermal resistance  thermal conductivity  Design value of thermal conductivity |  | m²·K/W  W/m·K  W/m·K |
| Raw density1) or raw density range |  | kg/m3 |
| Euro class of fire behavior according to ÖNORM EN 13501-1 | E |  |
| Dimensional stability in normal climate | level |  |
| Dimensional stability under defined temperature and humidity conditions | class |  |
| Upper application limit temperature | level |  |
| Lower application limit temperature | level |  |
| Compressive stress at 10% compression | level |  |
| flexural strength | level |  |
| Tensile strength perpendicular to the plane of the plate | level |  |
| Long-term creep behaviour under compressive stress | level |  |
| Water absorption during long-term immersion | level |  |
| Long-term water absorption by diffusion | level |  |
| Freeze-thaw cycling | passed |  |
| Water vapor diffusion resistance factor µ or  water vapor diffusion resistance Z |  | -  m²·s·Pa/kg |
| Dynamic Stiffness | level |  |
| Long-term thickness reduction | level |  |
| Small amounts of water-soluble ions: chloride, fluoride, silicate and sodium ions | levels |  |
| pH value | Permissible Deviations |  |

1. Mean bulk density

For specific EPD the technical data of the product must be declared as required in Tables 4 and 5.

For average EPD (“Sector or Branch-EPD“, “Group EPD” or “EPD from Associations”) Tables 4 and 5 must be filled, average values or ranges are accepted, in addition a note stating „see product sheets“ pointing to single technical product sheets can be cited. Technical data must be provided by the manufacturers. The manufacturers are to ensure that the relevant data are accessible, and the LCA-practitioner must indicate the sources where the technical data can be downloaded.

In this case the average value of nominal density/ weight per m² used for calculating the LCA must be declared as an additional information in chapter 3.1.

Note:

When averaging, it should be taken into account that, with regard to possible grouping into classes, the gross density is more decisive than the application according to EN 16783.

In case of declaring average values ÖNORM EN 16783 chapter 6.3.6 must be considered:

Grouping of products and declaring average values is allowed without reporting differences,

if the differences in each impact category are lower than 25 %. In other cases, the differences in the

impact categories shall be reported together with average values.

## Basic/auxiliary materials

The product components and/or contents and ingredients must be declared in mass-% to enable the user of the EPD to understand the composition and structure of the product in delivery status. These indications shall also support security and efficiency in installation, use and disposal of the product.

The declaration of mass-% can be accurate numbers or a range by analogy with REACH[[1]](#footnote-1) . The mass of components that make up less than 1 mass-% of the total product mass can be declared with < 1 mass-%.

The declaration of material product content must list at least those substances contained in the product which are included in the “Candidate List of Substances of Very High Concern for Authorization” where their contents exceed the limit values (0.1 mass-% on product level) for registration by the European Chemicals Agency (ECHA[[2]](#footnote-2)). If substances and preparations lose their hazardous features during manufacturing (e.g. after a complete chemical reaction) they are exempted from the obligation of declaration.

If the content of the material is below the limit of ECHA the following note must be stated in the EPD:

„The content of XXXX is below the limit values of the registration by the European Chemicals Agency (ECHA). Interpreting statements such as “… free of …” or “… are entirely harmless …” are not permissible.

The product components must be described in detail, so that their sort of product is clear, but the protection of sensitive data is assured, and company secrets are not revealed.

For additives, the function and substance class respective chemical group (i.e. hydraulic binders) must be stated. In addition to that all auxiliary materials and additives that stay within the product must be declared.

**Specific notes for the creation of an EPD for EPS and XPS insulating materials:**

Table 6: base materials in mass-% (example)

|  |  |  |  |
| --- | --- | --- | --- |
| **Components** | **CAS** | **Function** | **Mass fraction in percent** |
| PS granules x) |  |  |  |
| Designation of other components, e.g. EPS recyclate x) |  |  |  |
| e.g. silicate coating x) |  | e.g. protection against solar radiation |  |

Description of the manufacturing process of the PS granules

List of the ingredients in the PS granules including function and quantity in % by mass in Table 6.

Table 7: Basic materials in PS granules (example)

|  |  |  |  |
| --- | --- | --- | --- |
| **Components** | **CAS** | **Function** | **Mass fraction in percent** |
| Polystyrole x) |  | main ingredient |  |
| z.B. PolyFR x) |  | e.g. flame retardants |  |
| z.B. Pentane x) |  | e.g. propellant |  |
| z.B. Graphite x) |  | e.g. infrared absorbers |  |

Optional: footnote with description for each component

x)

x)

**Auxiliaries / additives**

Specifications and proportions of excipients are to be stated (in text or tabular format)

## Production

The process of production must be described and illustrated with a simple figure (i.e. flow chart). In case of average EPD the production processes of all sites must be described respective a useful summary must be included and a list of all production sites must be provided in an annex. Quality management systems, eco management systems etc. can be referred to.

**Specific notes for the creation of an EPD for EPS and XPS insulating materials:**

Description of raw material extraction, processing and geographical origin of raw materials, special processing chains….

Example of flow chart/graphic

Figure 1: Example of a flow chart/graphic production stage

Insulation materials made from expanded polystyrene rigid foam are manufactured in a three-stage process:

In the pre-expansion plant, the EPS beads are exposed to steam at around 100 to 110 °C. The polystyrene softens, the pentane vapor pressure increases and the EPS beads expand into foam balls. The contained nucleating agents are responsible for the foam structure.

The most commonly used process for the production of insulating panels is block foaming with subsequent cutting. After foaming, the foam particles are cooled and temporarily stored in silos. Cooling reduces the vapor pressure of the pentane and the water involved. A negative pressure is created in the beads. Air diffuses into the particles while water vapor and pentane escape from the particles. The interim storage lasts about a day. In the third process step, the foam particles are filled into molds (usually cuboid block molds) and foamed with steam at 100 to 120 °C. This leads to further expansion and welding of the particles to form the molded part. The molds are cooled with water and, after a stabilization period, the EPS blocks are removed from the mold. Finally, the blocks are cut into slabs. Edge profiles such as tongue and groove or shiplap can be created by milling.

Panels as molded parts (automatic panels) are produced in molding machines. The finished panels are immediately available in the desired final shape, e.g. folded.

## Packaging

Information concerning each component of packages:

Type (Foil, pallets, etc.),

Material (Paper, Polyethylene; including origin, e.g. recycled paper) and

Possibilities of reuse (e.g. multi way pallets).

**Specific notes for the creation of an EPD for EPS and XPS insulating materials:**

Example: The products are packed in a polyethylene film (PE-LD, 50-70 µm) and delivered on reusable pallets.

## Conditions of delivery

Written description of conditions of delivery, units of delivery, size and dimension as well as requirements on storage important for the declared product(s). Example: rolls, slabs or mats.

## Transport

Description of delivery (Route and means of transport).

## Processing/ installation

Description of way of treatment, used machines, tools, dust collection etc., auxiliary materials as well as measures of noise reduction. Notes regarding [recognized](http://www.dict.cc/englisch-deutsch/recognized.html) [rules](http://www.dict.cc/englisch-deutsch/rules.html) [of](http://www.dict.cc/englisch-deutsch/of.html) [engineering](http://www.dict.cc/englisch-deutsch/engineering.html), work safety or protection of the environment can be included.

References to detailed processing directives and referrals to user safety (safe use instruction sheets) of the manufacturer are required.

**Specific notes for the creation of an EPD for EPS and XPS insulating materials:**

Installation scenarios for use in EIFS must be described in detail (components of system).

**Specific LCA calculation rules for EPS and XPS insulating materials:**

Installation scenarios for use in EIFS – allocation of material flows to be calculated in A1-A3 and those flows to be declared in A5 as per CEN TR 16970 = Guidance Document to EN 15804) must be described.

## Use stage

Notes describing specific features of the material composition relevant for the use stage.

**Specific notes for the creation of an EPD for EPS and XPS insulating materials:**

If insulating products are installed professionally and if the phase of utilization is not disturbed, no modifications of the material composition occur.

## Reference service life (RSL)

The indication of the reference service life (RSL) is imperative for EPDs covering the complete use stage (modules B1-B7), or if a use stage scenario is described, which refers to the lifetime of the product (“from cradle to grave”).

The RSL must refer to the declared technical and functional quality of the product. It must be established in line with all of the specific rules in the European product standards and must also take consideration of the ISO 15686-1, -2, -7 and -8 standards.

Where information is available for deriving the RSL from harmonized European product standards, such data has priority.

The assumption underlying the calculation of the RSL and for those only the RSL can be declared must be stated. Influence on aging as per recognized rules of engineering.

**Specific notes for the creation of an EPD for EPS and XPS insulating materials:**

Table 8: Reference service life (RSL)

|  |  |  |
| --- | --- | --- |
| **Characterization** | **value** | **unit** |
| EPS or XPS slabs |  | years |
| Reference conditions on which the RSL is based (if relevant) |  | Individual units |

See EN 15804+A2 clause 6.3.4 and Annex A requirements and guidelines for reference service life

If no reference service life can be determined according to the rules of EN 15804+A2 (Annex A), a default value from a complementary PCR of the CEN/TC product committees, if available, must be used. If no complementary PKR is available, the service life can be declared from service life catalogues, depending on the area of ​​application, stating the source, e.g. according to BAU EPD-M-DOKUMENT-20-Reference-usage-times-20150810 (Austria) or the BBSR table "Useful lives of components on life cycle analysis according to BNB” (Germany). If no information can be found there, the RSL can be derived from other sets of regulations (Eurocodes, other basis).

## Reuse and recycling

Possibilities and scenarios of reuse and recycling must be described.

## Disposal

The different ways of disposal must be described.

The EAK-waste disposal code (Disposal code following the European list of waste) must be declared.

## Further information

Optional details, indication of reference source for additional information, e.g. websites…

# LCA: Calculation rules

## Declared unit/ Functional unit

The declared resp. functional unit, the mass reference and the conversion factor to 1 kg must be declared in a table.

**Specific LCA calculation rules for EPS and XPS insulating materials:**

The declared unit is 1 cubic meter of insulating material (1 m³). The data can be added to a functional unit

(e.g. 1 m² of thermal insulation for a specific thermal insulation resistance (RD value) or 1 m of a thermal insulation material for a pipe section with a declared lambda value (thermal conductivity), diameter and thickness, as delivered or as used to insulate a pipe).

Table : Declared unit

|  |  |  |
| --- | --- | --- |
| **characterization** | **value** | **unit** |
| declared unit | 1 | m3 |
| gross density for conversion into kg |  | kg/m3 |

Table : Functional unit

|  |  |  |
| --- | --- | --- |
| **characterization** | **value** | **unit** |
| functional unit i.e. for RD = 1 m2K/W | 1 | m2 |
| Calculation factor for conversion into kg |  | - |

Table 11: Functional unit m(insulation for pipes)

|  |  |  |
| --- | --- | --- |
| **characterization** | **value** | **unit** |
| functional unit | 1 | m |
| Lambda-value |  | W/(m·K) |
| diameter |  | cm |
| Layer thickness |  | cm |
| Calculation factor for conversion into kg |  | kg/m |

If average results of different products are declared, the methods of calculating the average values must be explained.

In this case the average value of nominal density/ weight per unit used for calculating the LCA must be declared as an additional information.

## System boundary

The type of EPD with regard to the applied system boundaries must be specified in the EPD. All building products and materials must declare modules A1-A3, modules C1-C4 and module D. The following EPD types may be specified:

• from the cradle to the factory gate with modules C1-C4 and module D (A1-A3 + C + D);

• from the cradle to the factory gate with options, modules A1-A3, C1-C4 and D (A1-A3 + C + D and additional modules. The additional modules may be one or more modules selected from A4 to B7);

• from cradle to grave and module D (A + B + C + D)

Exceptions to this rule are specified in EN 15804+A2, chapter 5.2.

Note: The specifications for the modules that must be declared no longer correspond to ÖNORM EN 16783:2017 - the specifications from EN 15804:2019+A2 apply primarily.

All declared life cycle stages (modules) are to be marked with an "X" in Table 8. Undeclared modules are to be marked with ND (= not declared).

Table 12: Declared life cycle stages

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **PRODUCT STAGE** | | | **CON-STRUCTION PROCESS STAGE** | | **USE STAGE** | | | | | | | **END-OF-LIFE STAGE** | | | | **BENEFITS AND LOADS BEYOND THE SYSTEM BOUNDARIES** |
| A1 | A2 | A3 | A4 | A5 | B1 | B2 | B3 | B4 | B5 | B6 | B7 | C1 | C2 | C3 | C4 | D |
| Raw material supply | Transport | Manufacturing | Transport from the gate  to the site | Construction, installation | Use | Maintenance | Repair | Replacement | Refurbishment | Operational energy use | Operational water use | De-construction, demolition | Transport | Waste processing | Disposal | Reuse-  Recovery-  Recycling-  potential |
| x | x | x | x | x | x | x | x | x | x | x | x | x | x | x | x | x |

X = included in LCA; MND = Module not declared

The modules assessed in the LCA study must be described shortly. It should be made apparent, which processes are calculated in which module and how the system boundaries to nature resp. to other product systems are set (if relevant for the declared product).

If not all modules are declared in an EPD, a clear justification must be given.

**Specific LCA calculation rules for EPS and XPS insulating materials:**

**A1-A3**

• The minimum requirement for the creation of a product specific EPD is the life cycle inventory data from the preparation of the PS granulate to the EPS or XPS insulating material ready for delivery

• The use of generic data is permitted for balancing the raw materials (PS granulate, coating, etc.) if no process-specific data is available. The generic data set for the PS granules should be based on current industry data.

• It must be ensured that the data records are complete. In this context, special attention should be paid to process-specific VOC emissions.

• All pentane emissions are classified as A1-A3.

**A4-A5**

• Guidelines for material losses

o 10% of the delivery quantity for insulation panels for insulation of external walls

o 5% of the delivery quantity for insulating boards for insulating ceilings and roofs

o If lower values ​​are to be used, the manufacturer must provide evidence of this.

**B1-B7**

• B1 use: any emissions of propellant residues are already assigned to A1-3.

• B2 maintenance and B3 repairs: Thermal insulation materials do not require any maintenance or repair work under normal conditions and if they have been installed correctly. The environmental impacts are therefore “0” in the default scenario.

• The stage B4 replacement is equivalent to the end of product life. The environmental impacts are therefore “0” in the default scenario.

• Stages B5 conversion/renewal, B6 energy use and B7 water use are not applicable at insulation level. The environmental impacts are therefore “0” in the “Default Scenario”.

**C1 - C4 and D**

• When balancing the disposal phase, at least one scenario must contain thermal waste recycling or treatment of the insulating material. Further scenarios for recycling such as bound EPS fills can be described.

• Waste collection and treatment processes for thermal utilization within the product system are considered in C3 or C4 if the end of the waste has not been reached. If the energy efficiency rate of the incineration plant is > 60%, the treatment and recovery plant is to be calculated in C3, with rates < 60% in C4. In both cases, credits for the electricity and heat quantities received in Germany are possible.

• Specifications for offsetting reuse, recovery and recycling potential:

o For the provision of secondary raw materials, the credit is based on the effort required to provide the substituted raw material.

For the production of the substituted raw material, the effort must be used according to the existing market mix of primary and secondary material.

The alternative provision of gas should be used for thermal energy generated, and the national energy mix for electricity generated (see General Life Cycle Assessment Rules of Bau EPD GmbH).

## Flow chart of processes/stages in the life cycle

A meaningful flow chart describing the manufacturing process shall give further aid to comprehension. The flow chart must be subdivided at least into the phases of life cycle declared (production, use, end-of-life). The phases can be partitioned into appropriate process stages.

## Estimations and assumptions

The assumptions and assessments that are important for the interpretation of the life cycle assessment are to be listed here.

## Cut-off criteria

The application of the cut-off criteria according to MS-HB Chapter 5.5.3 must be documented here.

## Data sources

The quality of the collected data must be described.

## Data quality

The sources of the backround data sets must be declared. If necessary, additional information on the quality of the used data sets shall be made (estimations). The issuing year of the used data material must be indicated.

## Reporting period

The period under review must be documented (in case of average EPD this would be the basis of the calculated average).

## Allocation

The allocations of relevance for calculation (appropriation of expenses across various products) must be indicated, at least:

* System boundary settings/allocation in the use of recycled and/or secondary raw materials
* Allocation concerning co-products
* Allocation of energy, auxiliary and operating materials used for individual products in a factory
* Loads and credits from recycling or energy recovery of packaging materials and production waste
* Loads and credits from recycling or energy recovery from the end of life of the product

whereby reference must be made to the modules in which the allocations are performed.

Detailed regulations concerning calculation of secondary materials and allocation MS-HB chapter “LCA rules” apply in all studies.

## Comparability

With reference to comparability of EPD data the following facts must be mentioned:

Comparison or benchmarking of EPD data is only possible, if all compared data sets are calculating following EN 15804 in the same version, the same programme specific PCR-rules or other additional rules. The same backround data sources and software versions must be applied. Moreover, the context of the function in the building or product specific features of performance must be considered.

# LCA: Scenarios and additional technical information

The following information is mandatory to give for all declared modules, for modules not declared it is optional. If need, additional information can be declared.

## A1-A3 product stage

Following EN 15804 no scenario documentation is required for A1-A3 for the declaration and calculation of these modules lies within the responsibility of the manufacturer and must not be altered by the LCA practitioner.

Note: the masses of packaging per declared unit must be indicated, this is especially important if A5 is not declared.

## A4-A5 Construction process stage

Table 9 and the units listed must be used for calculation the environmental impact of the transport phase.

Table 10 and the units listed must be used for calculation the environmental impact of the installation into the building.

Table 13: Description of the scenario „Transport to building site (A4)“

|  |  |
| --- | --- |
| **Parameters to describe the transport to the building site (A4)** | **Quantity per unit** |
| Average transport distance | km |
| vehicle type, Commission Directive 2007/37/EC (European Emission Standard) | - |
| Fuel type and average consumption of vehicle | l/100 km |
| Maximum transport mass | tons |
| Capacity utilisation (including empty returns) | % |
| Bulk density of transported products | kg/m3 |
| Volume capacity utilisation factor (factor: =1 or <1 or ≥ 1 for compressed or nested packaged products) | - |

x) The table must be filled with reference to the information available from the datasets used (i.e. in case of transport by ship). The datasets used must be noted in a footnote.

Table 14: Description of the scenario „Installation of the product in the building (A5)“ as per table 8 in ÖNORM EN 15804

|  |  |
| --- | --- |
| **Parameters to describe the installation of the product in the building (A5)** | **Quantity per unit** |
| Ancillary materials for installation (specified by material); | Meaningful unit |
| Water use | m3 |
| Other resource use | kg |
| Electricity demand | kWh or MJ |
| Other energy carrier(s): ……………. | kWh or other unit (e.g. litres) |
| Wastage of materials on the building site before waste processing, generated by the product’s installation (specified by type) | kg |
| Output materials (specified by type) as result of waste processing at the building site e.g. of collection for recycling, for energy recovery, disposal (specified by route) | kg |
| Direct emissions to ambient air, soil and water | kg |

## B1-B7 use stage

Reference Service life: [a]

The parameters and the units listed in the following tables must be used for calculation the environmental impact of the use stage (B2-B7). The tables can be excluded if no input or output happens. In this case a note of explanation would be sufficient: “In module BX-BY no material resp. mass flows occur, input +/- output = 0

Table 15: Description of the scenario „maintenance (B2)“ based on table 9 in EN 15804

|  |  |  |
| --- | --- | --- |
| **Parameters maintenance (B2)** | **value** | **unit** |
| Maintenance process |  | Description or source where description can be  found |
| Maintenance cycle |  | Number per RSL or year a |
| Ancillary materials for maintenance, e.g.  cleaning agent, specify materials |  | Kg/cycle |
| Waste material resulting from maintenance (specify materials) |  | kg |
| Net fresh water consumption during maintenance |  | m3 |
| Energy input during maintenance, e.g. vacuum cleaning, energy carrier type, e.g. electricity, and amount, if applicable and relevant |  | kWh |

Table 16: Description of the scenario „repair (B3)“

|  |  |  |
| --- | --- | --- |
| **Parameters repair (B3)** | **value** | **unit** |
| Repair process |  | Description or source where description can be  found |
| Inspection process |  | Description or source where description can be  found |
| Repair cycle |  | Number per RSL or year |
| Ancillary materials, e.g. lubricant, specify  materials |  | Kg or kg/cycle |
| Waste material resulting from repair, (specify materials) |  | kg |
| Net fresh water consumption during repair |  | m3 |
| Energy input during repair, e.g. crane activity,  energy carrier type, e.g. electricity, and amount |  | kWh |

Table 17: Description of scenario „replacement (B4)“

|  |  |  |
| --- | --- | --- |
| **Parameters replacement (B4)** | **value** | **unit** |
| Replacement cycle |  | Number per RSL or year |
| Energy input during replacement e.g. crane  activity, energy carrier type, e.g. electricity and  amount if applicable and relevant |  | kWh |
| Exchange of worn parts during the product’s life cycle, e.g. zinc galvanised steel sheet, specify materials |  | kg |
|  |  |  |

Table 18: Description of scenario „refurbishment (B5)“

|  |  |  |
| --- | --- | --- |
| **Parameters refurbishment (B5)** | **value** | **unit** |
| Refurbishment process |  | Description or source where description can be  found |
| Refurbishment cycle |  | Number per RSL or year |
| Energy input during refurbishment e.g. crane  activity, energy carrier type, e.g. electricity, and  amount if applicable and relevant |  | kWh |
| Material input for refurbishment, e.g. bricks, including ancillary materials for the refurbishment process e.g. lubricant, (specify materials) |  | kg or kg / cycle |
| Waste material resulting from refurbishment (specify materials) |  | kg |
| Further assumptions for scenario development, e.g. frequency and time period of use, number of occupants |  | Units as appropriate |

Table 19: Description of scenarios „energy (B6)“ resp. „Water (B7)“

|  |  |  |
| --- | --- | --- |
| **Parameters energy (B6) and water (B7)** | **value** | **unit** |
| Ancillary materials, e.g. lubricant, specify  materials |  | Kg or kg/cycle |
| Net fresh water consumption |  | m3 |
| Type of energy carrier, e.g. electricity, natural gas, district  heating |  | kWh or m³ |
| Power output of equipment |  | kW |
| Characteristic performance, e.g. energy efficiency, emissions, variation of performance with capacity utilisation etc. |  | units as appropriate |
| Further assumptions for scenario development, e.g. frequency and period of use, number of occupants |  | units as appropriate |

**Specific LCA calculation rules for EPS and XPS insulating materials:**

For EPS and XPS insulating materials no LCA-relevant material- and energy flows occur in use stage (B1). Therefore results in B1 must be declared with “0”.

During use stage no processes with regard to maintenance, repair or replacement and refurbishment occur, therefore no environmental impact is to calculate in modules B2-B5 (the results must be declared with “0”). Modules B6 and B7 are not relevant for insulating materials, with that no impact is to calculate ( B6 and B7 must be declared with “0”).

## C1-C4 End-of-Life stage

Short description of processes concerning disposal and scenarios going with that (i.e. for transport).

**Specific LCA calculation rules for EPS and XPS insulating materials:**

Existing processes of treatment should be described, even if technical or economic framework conditions make treatment not sensible at the time of publication of the EPD.

Table 20: Description of the scenario „Disposal of the product (C1 to C4)“ according to table 12 in EN 15804

|  |  |  |
| --- | --- | --- |
| **Parameters for End-of-Life stage (C1-C4)** | **value** | **Quantity per m3 insulation material** |
| Collection process specified by type |  | kg collected separately |
|  | kg collected with mixed construction waste |
| Recovery system specified by type |  | kg for re-use |
|  | kg for recycling |
|  | kg for energy recovery |
| Disposal specified by type |  | kg product or material for final deposition |
| Assumptions for scenario development, e.g. transportation |  | Appropriate units |

## D Potential of reuse and recycling

Short description of assumptions for reuse-, recover- and recycling processes.

**Specific LCA calculation rules for EPS and XPS insulating materials:**

Any substitutions of primary materials with regards to any considered share of secondary materials from insulating materials removed in C1 must be declared in module D (net flows).

Table 21: Description of the scenario „re-use, recovery and recycling potential (module D)“

(Substituted primary materials resp. technologies must be declared in a separate footnote (including technical information).

|  |  |  |
| --- | --- | --- |
| **Parameters for module D** | **value** | **unit** |
| Materials for reuse, recovery or recycling from A4-A5 |  | % |
| Energy recovery or secondary fuels from A4-A5 |  | MJ/t resp. kg/t |
| Materials for reuse, recovery or recycling from B2-B5 |  | % |
| Energy recovery or secondary fuels from B2-B5 |  | MJ/t resp. kg/t |
| Materials for reuse, recovery or recycling from C1-C4 |  | % |
| Energy recovery or secondary fuels from C1-C4 |  | MJ/t resp. kg/t |

# LCA: results

The declaration of environmental indicators must be listed in the following tables with reference only to the declared life cycle stages. Indicator values should be declared with three valid digits (eventually exponential form (e.g. 1.23E-5 = 0.0000123). A uniform format should be used for all values of one indicator. It is preferred that the definitions of the environmental indicators are spelled out completely to ensure the best possible readability. If space is needed in case of too many columns the defined abbreviations are accepted.

Note: ÖNORM EN 16783 Section 6.3.6 applies when specifying averages:

Groupings of substances and declaration of mean values ​​are acceptable without stating differences if the differences in each impact category are less than 25%. In other cases, the differences in the impact categories must be given together with mean values.

Table 22: Parameters to describe the environmental impact of mineral insulating products per declared/functional unit

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Para-meter** | **unit** | **A1-A3** | **A4** | **A5** | **B1** | **B2** | **B5** | **B6** | **B7** | **C1** | **C2** | **C3** | **C4** | **D** |
| GWP total | kg CO2 eq. |  |  |  |  |  |  |  |  |  |  |  |  |  |
| GWP fossil fuels | kg CO2 eq. |  |  |  |  |  |  |  |  |  |  |  |  |  |
| GWP biogenic | kg CO2 eq. |  |  |  |  |  |  |  |  |  |  |  |  |  |
| GWP luluc | kg CO2 eq. |  |  |  |  |  |  |  |  |  |  |  |  |  |
| ODP | kg CFC-11 eq. |  |  |  |  |  |  |  |  |  |  |  |  |  |
| AP | mol H+ eq. |  |  |  |  |  |  |  |  |  |  |  |  |  |
| EP freshwater | kg PO43- eq. |  |  |  |  |  |  |  |  |  |  |  |  |  |
| EP marine | kg N eq. |  |  |  |  |  |  |  |  |  |  |  |  |  |
| EP terrestrial | mol N eq. |  |  |  |  |  |  |  |  |  |  |  |  |  |
| POCP | kg NMVOC eq. |  |  |  |  |  |  |  |  |  |  |  |  |  |
| ADPE | kg Sb eq. |  |  |  |  |  |  |  |  |  |  |  |  |  |
| ADPF | MJ Hu |  |  |  |  |  |  |  |  |  |  |  |  |  |
| WDP | m3 Welt eq. entz. |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Legende | | GWP = Global warming potential; luluc = land use and land use change;  ODP = Depletion potential of the stratospheric ozone layer; AP = Acidification potential, Accumulated Exceedance; EP = Eutrophierungspotenzial; EP = Eutrophication potential; POCP = Formation potential of tropospheric ozone photochemical oxidants;  ADPE = Abiotic depletion potential for non-fossil resources; ADPF = Abiotic depletion potential for fossil resources WDP = Water (user) deprivation potential, deprivation-weighted water consumption | | | | | | | | | | | | |

Table : Additional environmental indicators

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Parameter** | **Unit** | **A1-A3** | **A4** | **A5** | **B1** | **B2** | **B5** | **B6** | **B7** | **C1** | **C2** | **C3** | **C4** | **D** |
| PM | disease incidence |  |  |  |  |  |  |  |  |  |  |  |  |  |
| IRP | kBq U235 eq. |  |  |  |  |  |  |  |  |  |  |  |  |  |
| ETP-fw | CTUe |  |  |  |  |  |  |  |  |  |  |  |  |  |
| HTP-c | CTUh |  |  |  |  |  |  |  |  |  |  |  |  |  |
| HTP-nc | CTUh |  |  |  |  |  |  |  |  |  |  |  |  |  |
| SQP | dimension-less |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Legende | | PM = Potential incidence of disease due to Particulate Matter emissions; IRP = Potential Human exposure efficiency  relative to U235; ETP-fw = Potential Comparative Toxic Unit for ecosystems; HTP-c = Potential Comparative Toxic Unit for humans – cancer effect; HTP-nc = Potential Comparative Toxic Unit for humans – non-cancer effect; SQP = Potential soil quality index | | | | | | | | | | | | |

Table 24: Parameters to describe the use of resources of mineral insulating products per declared/functional unit

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Para-meter** | **unit** | **A1-A3** | **A4** | **A5** | **B1** | **B2** | **B5** | **B6** | **B7** | **C1** | **C2** | **C3** | **C4** | **D** |
| PERE | MJ, net calorific value |  |  |  |  |  |  |  |  |  |  |  |  |  |
| PERM | MJ, net calorific value |  |  |  |  |  |  |  |  |  |  |  |  |  |
| PERT | MJ, net calorific value |  |  |  |  |  |  |  |  |  |  |  |  |  |
| PENRE | MJ, net calorific value |  |  |  |  |  |  |  |  |  |  |  |  |  |
| PENRM | MJ, net calorific value |  |  |  |  |  |  |  |  |  |  |  |  |  |
| PENRT | MJ, net calorific value |  |  |  |  |  |  |  |  |  |  |  |  |  |
| SM | kg |  |  |  |  |  |  |  |  |  |  |  |  |  |
| RSF | MJ, net calorific value |  |  |  |  |  |  |  |  |  |  |  |  |  |
| NRSF | MJ, net calorific value |  |  |  |  |  |  |  |  |  |  |  |  |  |
| FW | m3 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Legend | | PERE = Renewable primary energy as energy carrier; PERM = Renewable primary energy resources as material utilization; PERT = Total use of renewable primary energy resources; PENRE = Non-renewable primary energy as energy carrier; PENRM = Non-renewable primary energy as material utilization; PENRT = Total use of non-renewable primary energy resources; SM = Use of secondary material;  RSF = Use of renewable secondary fuels; NRSF = Use of non-renewable secondary fuels;  FW = Use of fresh water | | | | | | | | | | | | |

contains restrictions that must be declared according to the following classification in the project report and in the EPD with regard to the declaration of relevant core and additional environmental impact indicators.

Table 25 contains restrictions that must be declared according to the following classification in the project report and in the EPD with regard to the declaration of relevant core and additional environmental impact indicators.

Table 25: Classification of disclaimers to the declaration of core and additional environmental impact indicators

|  |  |  |
| --- | --- | --- |
| **ILCD-classification** | **Indicator** | **Disclaimer** |
| ILCD-Type 1 | GWP Global Warming Potential | none |
| ODP Ozone Depletion Potential | none |
| PM Particulate Matter | none |
| ILCD-Type 2 | Acidification potential, Accumulated Exceedance (AP) | none |
| Eutrophication potential, Fraction of nutrients reaching  freshwater end compartment (EP-freshwater) | none |
| Eutrophication potential, Fraction of nutrients reaching  marine end compartment (EP-marine) | none |
| Eutrophication potential, Accumulated Exceedance  (EP-terrestrial) | none |
| Formation potential of tropospheric ozone (POCP) | none |
| Potential Human exposure efficiency relative to U235 (IRP) | 1 |
| ILCD-Type 3 | Abiotic depletion potential for non-fossil resources  (ADP-minerals&metals) | 2 |
| Abiotic depletion potential for fossil resources (ADP-fossil) | 2 |
| Water (user) deprivation potential, deprivation-weighted  water consumption (WDP) | 2 |
| Potential Comparative Toxic Unit for ecosystems (ETP-fw) | 2 |
| Potential Comparative Toxic Unit for humans (HTP-c) | 2 |
| Potential Comparative Toxic Unit for humans (HTP-nc) | 2 |
| Potential Soil quality index (SQP) | 2 |
| Disclaimer 1 – This impact category deals mainly with the eventual impact of low dose ionizing radiation on human health of the nuclear fuel cycle. It does not consider effects due to possible nuclear accidents, occupational exposure nor due to radioactive waste disposal in underground  facilities. Potential ionizing radiation from the soil, from radon and from some construction materials  is also not measured by this indicator. | | |
| Disclaimer 2 – The results of this environmental impact indicator shall be used with care as the  uncertainties on these results are high or as there is limited experienced with the indicator. | | |

Table 26: Parameters describing LCA-output flows and waste categories of mineral insulating products per declared/functional unit

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Para-meter** | **unit** | **A1-A3** | **A4** | **A5** | **B1** | **B2** | **B5** | **B6** | **B7** | **C1** | **C2** | **C3** | **C4** | **D** |
| HWD | kg |  |  |  |  |  |  |  |  |  |  |  |  |  |
| NHWD | kg |  |  |  |  |  |  |  |  |  |  |  |  |  |
| RWD | kg |  |  |  |  |  |  |  |  |  |  |  |  |  |
| CRU | kg |  |  |  |  |  |  |  |  |  |  |  |  |  |
| MFR | kg |  |  |  |  |  |  |  |  |  |  |  |  |  |
| MER | kg |  |  |  |  |  |  |  |  |  |  |  |  |  |
| EEE | MJ |  |  |  |  |  |  |  |  |  |  |  |  |  |
| EET | MJ |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Legend | | HWD = Hazardous waste disposed; NHWD = Non-hazardous waste disposed; RWD = Radioactive waste disposed;  CRU = Components for re-use; MFR = Materials for recycling; MER = Materials for energy recovery; EEE = Exported electric energy; EET = Exported thermal energy | | | | | | | | | | | | |

Table 27: Information for description biogenic carbon content at factory gate

|  |  |
| --- | --- |
| **Biogenic carbon content** | **unit** |
| Biogenic carbon content in the product | kg C |
| Biogenic carbon content of packing | kg C |
| Note: 1 kg biogenic carbon is equivalent to 44/12 kg CO2 | | |

If the mass of biogenic carbon containing materials in the product is less than 5 % of the mass of the

product, the declaration of biogenic carbon content may be omitted.

If the mass of biogenic carbon containing materials in the packaging is less than 5 % of the total mass of

the packaging, the declaration of the biogenic carbon content of the packaging may be omitted.

# LCA: Interpretation

For better understanding of the LCA, the aggregated indicators of the inventory analysis as well as those of the impact assessment (LCIA) from chapter 5 must be interpreted in a dominance analysis. The interpretation must describe a range resp. variance of LCIA results, if the EPD is valid for more than one product.

It is recommended to illustrate the results with graphic elements (i.e. the dominance analysis showing distribution of environmental impacts over several modules…)

When declaring average products, the range of possible results for the individual products for the main impact categories that are relevant to the materials used must be specified.

As for module D, the interpretation must declare, that the benefits and loads lie beyond the system boundary. Any graphic elements showing result interpretation of the life cycle must be created in a way, that modules A1-C4 and module D are displayed separate picture elements. Alternatively, the results can be interpreted without graphic elements.

**Extension of an EPD:**

**It is mandatory to declare in a separate block in the project report:**

**Reasons for deviations of results of single indicators of more than 15% compared to the results before. This serves as an information for verifiers and enhances legal compliance. Users of the data can be informed of such facts.**

**Claims that can be published (i.e. same framework conditions, different electricity mix) can be declared in the EPD, if desired.**

# Literature

Relevant standards and sources for the preparation of the EPD resp. for the definition of the product must be listed here. The full documentation of references is to be done as follows:

Author, First name. and Author, First name. (year). Title of article. subtitle. location: publishing company.

Author, First name. (year). Title of article. In: Surname, First name. and Surname, First name. (Publishing company): Name of paper. Bd. 2 *or year number,* 207-210.

Organisation (Year): Full name of standard or rule. Date of Issue. Location. Legal institution.

Always to be quoted:

ÖNORM EN 13162: Thermal insulation products for buildings - Factory made EPS or XPS (MW) products - Specification

ÖNORM EN ISO 14040 Environmental management - Life cycle assessment -- Principles and framework

ÖNORM EN ISO 14044 Environmental management - Life cycle assessment -- Requirements and guidelines

ÖNORM EN ISO 14025 Environmental labels and declarations -Type III environmental declarations -- Principles and procedures

ÖNORM EN 15804 Sustainability of construction works - environmental product declarations. Core rules for the product category of construction products

ÖNORM 16783-Thermal insulation products ― Product category rules (PCR) for factory made and in-situ formed products for preparing environmental product declarations

Management system handbook including applicable documents from Bau EPD GmbH

# Directory and Glossary

## List of figures

[Figure 1: Example of a flow chart/graphic production stage 15](#_Toc517348360)

## List of tables

[Table 1: Applications for thermal insulation in buildings according to ÖNORM EN 16783 - Annex A 10](#_Toc98057549)

[Table 2: Applications for thermal insulation in building equipment, industry and civil engineering as per ÖNORM EN 16783 – Annex A 10](#_Toc98057550)

[Table 3: Product specific standards 11](#_Toc98057551)

[Table 4: Technical characterizations for products as per ÖNORM EN 13163 11](#_Toc98057552)

[Table 5: Technical data for products as per ÖNORM EN 14309 12](#_Toc98057553)

[Table 6: base materials in mass-% (example) 14](#_Toc98057554)

[Table 7: Basic materials in PS granules (example) 14](#_Toc98057555)

[Table 8: Reference service life (RSL) 16](#_Toc98057556)

[Table 9: Declared unit 18](#_Toc98057557)

[Table 10: Functional unit 18](#_Toc98057558)

[Table 11: Functional unit m(insulation for pipes) 18](#_Toc98057559)

[Table 12: Declared life cycle stages 19](#_Toc98057560)

[Table 13: Description of the scenario „Transport to building site (A4)“ 21](#_Toc98057561)

[Table 14: Description of the scenario „Installation of the product in the building (A5)“ as per table 8 in ÖNORM EN 15804 21](#_Toc98057562)

[Table 15: Description of the scenario „maintenance (B2)“ based on table 9 in EN 15804 22](#_Toc98057563)

[Table 16: Description of the scenario „repair (B3)“ 22](#_Toc98057564)

[Table 17: Description of scenario „replacement (B4)“ 22](#_Toc98057565)

[Table 18: Description of scenario „refurbishment (B5)“ 22](#_Toc98057566)

[Table 19: Description of scenarios „energy (B6)“ resp. „Water (B7)“ 23](#_Toc98057567)

[Table 20: Description of the scenario „Disposal of the product (C1 to C4)“ according to table 12 in EN 15804 23](#_Toc98057568)

[Table 21: Description of the scenario „re-use, recovery and recycling potential (module D)“ 24](#_Toc98057569)

[Table 22: Parameters to describe the environmental impact of mineral insulating products per declared/functional unit 25](#_Toc98057570)

[Table 23: Additional environmental indicators 25](#_Toc98057571)

[Table 24: Parameters to describe the use of resources of mineral insulating products per declared/functional unit 26](#_Toc98057572)

[Table 25: Classification of disclaimers to the declaration of core and additional environmental impact indicators 27](#_Toc98057573)

[Table 26: Parameters describing LCA-output flows and waste categories of mineral insulating products per declared/functional unit 28](#_Toc98057574)

[Table 27: Information for description biogenic carbon content at factory gate 28](#_Toc98057575)

## Abbreviations

### Abbreviations as per ÖNORM EN 15804

EPD environmental product declaration

PCR product category rules

LCA life cycle assessment

LCI life cycle inventory analysis

LCIA life cycle impact assessment

RSL reference service life

ESL estimated service life

EPBD Energy Performance of Buildings Directive

GWP global warming potential

ODP depletion potential of the stratospheric ozone layer

AP acidification potential of soil and water

EP eutrophication potential

POCP formation potential of tropospheric ozone

ADP abiotic depletion potential

### Abbreviations as per PCR on hand

CE-mark french: Communauté Européenne or Conformité Européenne = EC certificate of conformity

REACH Registration, Evaluation, Authorisation and Restriction of Chemicals

|  |  |  |
| --- | --- | --- |
|  | **Owner and Publisher**  Bau EPD GmbH  Seidengasse 13/3  1070 Wien  Österreich | Tel +43 699 15 900 500  Mail [office@bau-epd.at](mailto:office@bau-epd.at)  Web www.bau-epd.at |
|  | **Programme Operator**  Bau EPD GmbH  Seidengasse 13/3  1070 Wien  Österreich | Tel +43 699 15 900 500  Mail [office@bau-epd.at](mailto:office@bau-epd.at)  Web www.bau-epd.at |
| Logo | **Author of the Life Cycle Assessment**  Name of creator in person  Name of Institution (if rel.)  Address  Postcode, Location | Mail Person creator  Tel  Fax  Mail  Web |
| Logo | **Holder of the declaration**  Name of creator in person  Name of Institution (if rel.)  Address  Postcode, Location | Tel  Fax  Mail  Web |
|  |  |  |

1. **Regulation (EC) No 1907/2006 of the European Parliament and of the Council of 18 December 2006 concerning the Registration, Evaluation, Authorisation and Restriction of Chemicals (REACH), establishing a European Chemicals Agency, amending Directive 1999/45/EC and repealing Council Regulation (EEC) No 793/93 and Commission Regulation (EC) No 1488/94 as well as Council Directive 76/769/EEC and Commission Directives 91/155/EEC, 93/67/EEC, 93/105/EC and 2000/21/EC** [↑](#footnote-ref-1)
2. European Chemicals Agency: <http://echa.europa.eu/de> [↑](#footnote-ref-2)